### Please Note: This list is to be used as a quick reference guide to identify current models only.

### VIKING PROFESSIONAL COOKING

**C – At beginning of model number denotes Brigade products**

## **Ranges**

**V** –Viking Professional Series

**G** –Gas, **D**-Dual fuel, **E**-Electric, **I**- Induction

**S –** Self-clean/24"D, **C**- Infrared broiler/24”D.

**C –** Convection

**R**-- Range

**5** – Series **7**-Series

**30** –30"W, 36"W, 48"W,60"W

**4B** – 4 Burners, **4G**-4 Burners/Griddle, **6B**-6 Burners, **6G**-6 Burners/Griddle, **6GQ**-6 Burners/Griddle/Char-Grill, **8B**-8 Burners

\* Add LP after color code for factory conversion

### Rangetops

**V** –Viking Professional Series

**G** –Gas,

**R** –Range,

**T** –Top

**5** – Series **7**-Series

**30** –30”W, 36”W, 48”W

**4B** – 4 Burners, **4G**-4 Burners/Griddle,, **6B**-6 Burners, **6G**-6 Burners/Griddle,

\* Add LP after color code for factory conversion

### Cooktops

**V** –Viking Professional Series

**G** –Gas, **E**-Electric, **I**-Induction

**C** – Cooktop

**U** - Unit

**5** – Series

**30**–30”W **36**-36"W,

**5B** – 5 Burners, **6B**-6 Burners

\* Add LP after color code for factory conversion

Ovens

**V** – Viking Professional Series

**E**-- Electric

**S** – Single, **D**-Double

**O** –Oven

**F –**French Door

**1** – Select Oven, **5-**Premiere Oven, **7**-Series

**27** –27", **30**-30"

**2** – Digit change for new revisions

**Microwave Ovens**

**V** – Viking Professional Series

**M** –Microwave,

**C** –Combi, **S** –Steam

**O** –Oven, **TK**-Trim kit

**S** –Standard

**C** – Convection

**R** – Microwave Hood

**D** – DrawerMicro

**20** – 20”W, 36”W

**1** – Conventional, **5 or 6** – Convection

Warming Drawers

**V** –Viking Professional Series

**E** –Electric with door panel,

**W** –Warming

**D** –Drawer

**O** –Outdoor unit

**5** – Series

**30** – 30"W, **36**-36"W

### VIKING PROFESSIONAL VENTILATION

### Hoods

**V** – Viking Professional Series

**C** – Chimney **WH** –Wall Hood, **IH**-Island Hood **B**-Built-in, **CV**-Custom Ventilator **O**-Outdoor

**5 -** Series

**24** –24”W,30"W, 36"W, 42”W, 48”W, 54”W, 60”W, or 66”W

**1** –21”D, **4**-24”D, **7**-27”D, **0**-30”D

**0** –10”H, **8**-18”H **12-**12” H

**1** – Digit change for new revisions

### Downdraft

**V** – Viking

**DD** – Down Downdraft

**5** – Series

**30** – 30”W, 3**6**-36”W, 4**5**-45”W, 4**8**-48”W

**0**– Digit change for new revisions

###### **VIKING PROFESSIONAL REFRIGERATION**

# **Built-in and Freestanding Refrigerator/Freezers**

**V** –Viking Professional Series, **FD**-Full Overlay

**C** – Commercial style door

**S** – Side-by-side, **B**-Bottom mount, **W**-Wine celler, **R**-All Refrigerator, **F**-All Freezer or French Door

##### B – Built-in

**F** – Freestanding

**5** – “5” Series, “3” Series, “1” Series

**30** – 30”W, 36"W, 42”W, 48”W

**3** – Digit change for new revisions

\* For Bottom mount, all refrigerator/freezer models, add “**R**” or “**L**” to end of model number to signify the door hinge – right or left

#### Undercounter Refrigeration

**V** –Viking Professional Series,

**W** –Wine, **B**-Beverage, **R**-Refrigerator, **D**-Drawer

**U** –Undercounter,

**I** –Indoor, **O**-Outdoor

**5 -** Series

**24-**24", **15-**15”

**0** – Digit change for new revisions

**G** –Glass door **D** –Solid door,

\*Add “**R**” or “**L**” to end of all model numbers to signify door hinge – right or left (except refrigerated drawers)

VIKING PROFESSIONAL KITCHEN CLEANUP

# **Dishwasher**

**V** –Viking Professional Series

**F** – Full Overlay

**DW** – Dishwasher

**103**– Series

**302** - Series

**WS** – Water Softener

### VIKING PROFESSIONAL OUTDOOR

# **Viking Produced Grills**

**V** – Viking Professional Series

**G** – Gas

**B** – Bar-B, **I**-Infrared,

**Q** – Grill

**5** – Series,

**30** – 30”W, **36** – 36”W, **42** – 42”W, **54** – 54”W

**24 –** 24” Depth

**N** – Natural, **L**-LP/propane

Viking Produced Grill Cart

**B** – Bar-B

**Q** – Grill

**C** – Cart

**5** – Series

**30** – 30”W, **36** – 36”W, **42** – 42”W, **54** – 54”W

**1** – Digit change for new revisions

**Side Burners and Wok Cooker**

**V** –Viking Professional Series

**G** – Gas

**S** – Side

**B** –Burner

**WT** – Wok Top

**O** –Outdoor

**5 –** Series

**15** – 15”, **24** – 24”

**1 or 3** – Digit change for new revisions

# **Stainless Steel Cabinets**

**V** – Viking Professional

**Q** – BBQ, **B**-Base or Back, **U**-Undercounter, **S**-Sink or Side, **T**-Trash, **C**-Corner, **O**-Outer, **B** – Base, **W-**Warming Drawer Access, **R-**Refrigeration, **U**-Underneath Storage, **O** –Outdoor, **P**-Pullout or Panel, **C**-Corner, **F**-Filler

**O** – Outdoor

**4”** –4**, 16-**16”W, **18-**18”W, **24-**24”W, **26-**26”W, **30**-30”W, **32**-32”W, **36**-36”W, **41**-41”W, **53**-53”W, **90°**-90, **135°**-135

**0** – 0 drawers, **1**-1 drawer, **2**-2 drawers, **3**-3 drawers

**0** – 0 doors, **1**-1 door, **2**-2 doors

# **New 2017 Viking Grills**

**V** – Viking Professional Series

**Q** – Grill

**G** – Gas

**I**-Infrared

**FS** – Free Standing (comes with cart attached)

**5** – Series,

**30** – 30”W, **36** – 36”W, **42** – 42”W, **54** – 54”W

**0 –** Digit change for new revisions

**N** – Natural, **L**-LP/propane

**New 2017 Outdoor Side Burners/Power Burner/Warming Drawers**

**V** – Viking Professional Series

**Q** – Grill

**G** – Gas

**S** – Side

**B** –Burner

**PB** – Power Burner

**E** – Electric

**WD** – Warming Drawer

**5 –** Series

**13** – 13”, **20** – 20”, **30** – 30”, **42** – 42”

**0** – Digit change for new revisions

**New 2017 Viking Outdoor Access Door and Drawers**

**V** – Viking Professional Series

**O** – Outdoor

**A** – Access

**D** – Door

**R** – Drawer

**S** – Single

**D** - Double

**5 –** Series

**18** – 18”, **19** – 19”, **24** – 24”, **30** – 30”, **36** – 36”, **42** – 42”

### 0 – Digit change for new revisions

### VIKING 3 SERIES COOKING

**C – at beginning of model number denotes Brigade products**

## **Ranges**

**RV** – Viking 3 Series

**G** –Gas, **D**-Dual fuel, **E**-Electric

**R** – Range

**3** – Series

**30** –30"W

**1 or 2–** Digit Change

**5B** – 5 Burners

\* Add LP after color code for factory conversion

### Cooktops

**RV** – Viking 3 Series

**G** –Gas, **E**-Electric

**C** – Cooktop

**3** – Series

**30** –30”W **36**-36"W, 4**5**-45”W

**1** - Digit Change

**5B** – 5 Burners, **6B**-6 Burners

\* Add LP after color code for factory conversion

Ovens

**RV** – Viking 3 Series

**S** – Single, **D**-Double

**O** –Oven

**E**-Electric

**3** – Series

**30** – 30"

**Microwave Ovens**

**RV** – Viking 3 Series

**M** –Microwave

**H** – Microwave Hood

**C** – Convection

**TK**-Trim kit

**20** – 20”W, **30** –30”W

**3** – Series

Warming Drawers

**RV** – Viking 3 Series

**E** –Electric with door panel,

**W** –Warming

**D** –Drawer

**3** – Series

**30** – 30"W

### VIKING 3 SERIES VENTILATION

**Hoods**

**RV** – Viking 3 Series

**C** –Chimney

**H** – Hood

**3** – Series

**30** – 30"W, **36** – 36"W

###### **VIKING 3 SERIES REFRIGERATION**

# **Freestanding Refrigerator/Freezers**

**RV** – Viking 3 Series

**R** – Refrigerator

**F** **–** French Door

**3–** Series

**36** –36"W

VIKING 3 SERIES KITCHEN CLEANUP

# **Dishwasher**

**RV** – Viking 3 Series

**F** – Full overlay

**DW** – Dishwasher

**103**– Series

**302** - Series

**WS** – Water Softener

### VIKING TUSCANY

## **Ranges**

**T** –Tuscany

**V** –Viking

**D** – Dual fuel

**R** – Range

**36** – 36"W, 48"W,66"W

**0** – Digit Change

**4B** – 4 Burners, **2G**-2 Burners/Griddle, **4G**-4 Burners/Griddle, **4I**-4 Burners/Induction, **4F**-4 Burners/French Top, **2GI**-2 Burners/Griddle/Induction, **6B**-6 Burners, **6G**-6 Burners/Griddle, **8B**-8 Burners, **6I**-6 Burners/Induction

### Hoods

**T** –Tuscany

**V** –Viking

**W** –Wall

**H** – Hood

**36** – 36"W, 48”W, 66”W

**0** – Digit change for new revision

03/10/2017